REFERENCE         :   BERR_IN
AUTHOR            :   Clip Technology
CREATION DATE     :   01/06/95
VERSION NUMBER    :   ISaGRAF 3.32
REVISION NUMBER   :   2

DESCRIPTION :
Validation for buserror-handling:         
- input boards
The special buserror testboards create buserrors after 10 ... 20 cycles

MODIFICATIONS:
   DATE - AUTHOR - VER - REV : 01/06/95 - PEP Modular Computers - ISaGRAF 3.0 - 1
   DESCRIPTION   : 
   ---------------
   DATE - AUTHOR - VER - REV : 15/01/98 - Clip Technology - ISaGRAF 3.23 - 2
   DESCRIPTION   : 
   ---------------

