REFERENCE         :   POKWOTES
AUTHOR            :   Clip Technology
CREATION DATE     :   12/04/96
VERSION NUMBER    :   ISaGRAF 3.32
REVISION NUMBER   :   2

DESCRIPTION :
Example of using Function Block POK,  
 to write two bytes into target memory.
 The adress must be accessable, otherwise you'll get 'DISCONNECT'
 from the debugger and further you canīt use the ISaGraf-Kernel till you 
 delete and unlink ISA11.
 Important to know: The range for word is zero to 65535. 
 Other numbers are not allowed,

MODIFICATIONS:
   DATE - AUTHOR - VER - REV : 12/04/96 - PEP Modular Computers - ISaGRAF 3.0 - 1
   DESCRIPTION   : 
   ---------------
   DATE - AUTHOR - VER - REV : 15/01/98 - Clip Technology - ISaGRAF 3.23 - 2
   DESCRIPTION   : 
   ---------------

