REFERENCE         :   PEKBYTES
AUTHOR            :   Clip Technology
CREATION DATE     :   12/04/96
VERSION NUMBER    :   ISaGRAF 3.32
REVISION NUMBER   :   2

DESCRIPTION :
 Example of using Function Block PEEK
 to read one byte    from target memory.
 The address must be accessable, otherwise youŽll get 'DISCONNECT'
 from the debugger and further you can`t use the ISaGRAF-Kernel till yo
 delete and unlink ISA11.
 Important to know: The range for byte is zero to 255.
 Other Numbers are not allowed,

MODIFICATIONS:
   DATE - AUTHOR - VER - REV : 12/04/96 - PEP Modular Computers - ISaGRAF 3.0 - 1
   DESCRIPTION   : 
   ---------------
   DATE - AUTHOR - VER - REV : 15/01/98 - Clip Technology - ISaGRAF 3.23 - 2
   DESCRIPTION   : 
   ---------------

