REFERENCE         :   MEM_ABS
AUTHOR            :   Clip Technology
CREATION DATE     :   01/07/93
VERSION NUMBER    :   ISaGRAF 3.32
REVISION NUMBER   :   2

DESCRIPTION :
Absolute memory board validation.     
  First used address is on the DUAL-PORTED
  memory of a slave VSBC4 #1
  ($87408000)
  The semaphore access is also tested

******************************************************
* For PEP9000 systems, absolute memory areas have*
* been reserved:*
**
* -IUC9000:12 Kbytesfrom $20000 to $23000*
**
* -VME9000:12 Kbytesfrom $20000 to $23000*
**
* -VME9030:24 Kbytesfrom $D000A000 to $D0010000*
**
******************************************************

MODIFICATIONS:
   DATE - AUTHOR - VER - REV : 01/07/93 - PEP Modular Computers - ISaGRAF 3.0 - 1
   DESCRIPTION   : 
   ---------------
   DATE - AUTHOR - VER - REV : 15/01/98 - Clip Technology - ISaGRAF 3.23 - 2
   DESCRIPTION   : 
   ---------------

